DoubletCalc v1.4 release notes.

The functionality of this DoubletCalc release (DoubletCalc v1.4) is upgraded with the possibility to detail the well architecture. Additional input boxes are implemented to model the well tubings with varying diameters downhole. Additionally, the skin referring to a deviated well path as explained in the document "Effect scheve put.pdf" is now calculated in the program on basis of the input "penetration angle" http://www.nlog.nl/nl/geothermalEnergy/DoubletCalc.html). Finally, the input for the salinity now includes a min and a max value as well.
Other functionality remained the same. One is referred to the "handleiding DoubletCalc" for the technical and theoretical specifics.

In order to run DoubletCalc v1.4 standalone, Java version 1.6 or newer needs to be installed. Java can be downloaded from www.oracle.com. DoubletCalc is executed by clicking the file: DoubletCalc_v1_4.exe.

In the unlikely case the standalone doesn't execute, the batch file start.bat can be used as an alternative.

TNO 2013-10-07
